Basic Network Configuration
                                           Bob Samson, Mesa Community College, Mesa, AZ
	Network Address	Subnet Mask	1st usable	Last usable	Broadcast	
LAN-A  	192.168.12.0	255.255.255.0	.1	.254	.255	
LAN-B  	192.168.30.0	255.255.255.0	.1	.254	.255	

CABLING
Connect the correct cable types between the network devices and workstations. The numbers next to
a device indicates the port number to connect to. The light purple lines are not cables, merely guides.
When connecting to the PC, be sure to select the Fast-Ethernet port.

ROUTER and SWITCHES
The Router and Switches are already configured.

WORKSTATIONS
Select each PC and when the GUI box opens, choose the ‘Desktop Tab’. Choose the upper-left
option for ‘IP Configuration’. Using the address ranges above, enter proper values for:
•	IP Address
•	Subnet mask
•	Default-gateway
•	DNS address can be blank.

TESTING
Verify your configuration is correct by Pinging from each workstation to the other workstations.